**4ch H.264+ Wireless IP Kit**

**Features：**

* 720P/960P/1080P wireless network vedio recorder
* built in professional wifi moduel,strong singaland anti-interference ability
* no need match codeplug-play
* wired&wireless mix use,apply in different sense
* P2P esset，quick long-distance connect、smoothly image
* support muliti alarm trigger(vedio lost/motion detection)alarm output(sound/E-Mail)；
* support Android/Apple（or tablet PC）long distance（LAN\*NET）login and control



**Technical Speciﬁcation:**

|  |
| --- |
| **wireless NVR** |
| **model**  | KN7104W |
| **processore** | professional industrial processor  |
| **operation system**  | embed linux operation system |
| **video audio input** | network video input | 4 channel |
| **video output** | HDMI output | 1channel，resolution：1024x768, 1280x1024,1366x768, 1440x900,1920x1080p |
| VGA output | 1channel ，resolution：1024x768, 1280x1024,1366x768, 1440x900,1920x1080p |
| **video compression** | standard  H.264，H264+ |
| **video encoding specification** | recording resolution | 1080P/960P/720P |
| playback | 1 channel |
| **video manage** | recording/capture mode | manual recording、time recording 、motion detection recording、alarm recording |
| playback mode | instant playback、general playback、event playback |
| backup mode | general backup |
| **HDD drive** | type | 1 SATA connector |
| max capacity | every sata MAX 6TB |
| **eternal connector** | network port | one RJ45 10M/100M self adaptive ethernet port 2  antenna |
| USB port | 1 USB 2.0(2 USB port optional) |
| audio port | 1，3.5 inch headphone jack (optional） |
| **network management** | network protocol | UPnP（plug and play）、SMTP（email service）、PPPoE（dial up networking）、DHCP etc. |
|
| **Others** | power supply | DC 12V 2A |
| power consumption（without HDD） | ≤5W |
| working temperature | -10℃--＋55℃ |
| working humidity | 10％--90％ |
| size | 258×210×42mm |
| weight （no HDD） | ≤1Kg |
| **wireless IPC** |
| MODEL NUMBER | XZ-15T-HE | XZ-15T -HX | XZ-15T -HF9 |
| Structure | HI3518E+SC1145 | HI3518E+SC1135 | HI3516EV100+SC2235 |
| Mega Pixel | 100W | 130W | 200W |
| Max. Image Resolution | 1280X720 | 1280X960 | 1920X1080 |
| **processor** | professional industrial processor  |
| **operation system**  | embed linux operation system |
| **image sensor** | 1/3” Progressive Scan Sensor |
| **S/N Ratio** | > 39 dB |
| **video compression** | standard  H.264，H264+ |
| **Min illumination** | Color 0.001 Lux@ F1.2, Black-white 0.0001 Lux@F1.2 |
| **lens**  | 4mm |
| **white balance** | Auto |
| **Day & Night** | Auto / Color / BW |
| **3D-DNR** | Auto |
| **Mirror/Flip** | On / Off |
| **privacy masking**  | 4 Zone Selectable |
| **power input** | DC12V-1A |
| **power cocumption** | ≤6W |
| **connector** | reser button/ WIFI 802.11b/g/n |
| **working humidity/ temperature** | -10℃ to +50℃ / 30% to 80% RH |
| **Dimensions** | Φ105X80.8mm |